Life Science

Heal Force



OptiClean 900/1300

Vertical Laminar Flow Clean Benches



Heal Force Leads You to Healthier Life



[www.healforce.com](http://www.healforce.com)

Enhanced comfort and convenience

5 ° backward-slanted safety grade glass provides more comfortable viewing

Long life HEPA filter offers high separability for particles with high uniformity of air flow

Counterbalanced sliding sash is designed for easy operation with single hand.

Multiple levels of air flow speed are standard configured for wide range of applications

Universal wheels are designed for easy transportation

Advanced door lock guarantees your sample security to prevent unauthorized access

|  |  |  |
| --- | --- | --- |
|  | **OptiClean900** | **OptiClean1300** |
| Cleanliness in Work Area | ISO Class5, Class 100 (Fed 209E) |
| Prefilter | High efficiency polyester fibre |
| Main Supply Filter | HEPA with 99.99% Separability at 0.3um particle size |
| Veritical Airflow Velocity | 0.30 ~ | 0.60m/s(Adjustable) |
| Noise Emission | <65 dB(A) | <65 dB(A) |
| Fluorescent Light Intensity | >300 Lux | >300 Lux |
| Nominal Power | 300 VA | 550 VA |
| RMS | <5 um | <5 um |
| External Dimensions (WxDxH) | 1050x730 xl640mm | 1500x730x1640 mm |
| Internal Dimensions (WxDxH) | 950 x 650x510 mm | 1400x650 x 510 mm |
| Operator No. | One side for one person | One side for two persons |
| Net Weight | 110 Kg | 140 Kg |

**General Specifications, OptiClean Vertical Laminar Flow Clean Bench**

Heal Force Bio-Meditech Holdings Group

Heal Force International Trading(Shanghai) Co., Ltd

6788 Songze Road, Qingpu District, Shanghai 201706, P.R. China

Tel +86 21 62728646 Email export@healforce.com, Fax +86 21 62728646

Information is subject to change and/or updating without notice © 2020 Heal Force. For internal use only